Policy for new Garden of Remembrance

The area designated for the interment of cremated remains is shown on the attached map.

Cremated remains will be interred in sequence, forming two rows within the designated area, option 2 on the plan i.e starting at one end and working in pairs.

Cremated remains must be poured into the ground which is the preferred method according to Churchyard regulations. The size and nature of the area mean that caskets are not permitted. Pouring will also allow for a further interment in the same plot at a later date.

Memorial stones must be horizontal, 12” (30 cm) square, of polished black granite. These have embossed lettering which is easier to clean.

The design of the stone and the inscription must receive prior approval of the Rector. Additional inscriptions are permitted in the case of a further interment in the same plot.

The erection of any fencing or other form of demarcating the plot is not permitted.

Spike style flower vases may be used.

Available from [www.amazon.co.uk/plain-grave-flower-funeral](http://www.amazon.co.uk/plain-grave-flower-funeral)

The space between the stones will be covered in fine gravel